First pass design strategy

1. Find gain equation at each of the 4 stages
   1. Ignore ro, assume ro >> R1-4
2. Find RC time constaint at each node
   1. Ignore Cgd b/c Cgd = Cov << Cgs = 2/3WLCox + Cov
   2. Ignore bulk terminal caps b/c hard to estimate
3. Product of the 4 gains >= 30k. Allocate a percentage of 30k for each stage
4. 1/(sum of all nodes’ time constants) >= 90MHz. Allocate a percentage of 1/90Mhz for each node.
5. At this point, we have each stage’s gain in function of gm, R; each node’s time constant as a function of gm, R, C. We can correlate the 2 equations to assign values to gm, C, R variables.
6. From gm, we can find W.
7. After all xtors are sized, we will calculate Ids of the xtors connected to Vbias-Gen to determine the biasing voltage.

|  |  |  |  |
| --- | --- | --- | --- |
| Node | Time Constant | Assumptions/Simplifications | Simplified Time Constant |
| Input |  | * Cin >> Cgs2 |  |
| Vx |  | * R2/R1 < 4 |  |
|  |  |  |  |
|  |  |  |  |